;
; MEKA - Video Blitter configuration and modes
;
; [name]
; res = XRESOLUTIONxYRESOLUTION
; blitter = normal | double | scanlines | tvmode | eagle | parallel
; driver = auto | vga | modex | vesa1 | vesa2b | vesa2l | vesa3 | vesaaf
;
; Optional commands:
;  flip (enable page flipping to reduce color flickers, slow)
;  vsync (enable vertical synchronization to reduce flickers, very slow)
;
; Available video modes depends on your video card. Some modes you may
; want to try are 256x192, 256x240, 320x200 and 512x384.
;
; *FOR MAXIMUM PERFORMANCES*
; Set the higher VESA mode if possible as it's not always selected by
; default when using the "auto" driver.
;

[Normal]
res = 320x200
driver = auto

;[Vsync]
;res = 320x200
;vsync
;driver = auto

[Page Flipping]
res = 320x200
driver = auto
flip

;[VSync + Page Flipping]
;res = 320x200
;driver = auto
;vsync
;flip

;[Normal 256x192]
;res = 256x192
;driver = auto

[Doubled]
res = 512x384
blitter = double
driver = auto

;[Doubled Game Gear]
; res = 376x308
;; res = 320x350
;; res = 376x282
;; res = 360x360
;blitter = double
;driver = auto

[Scanlines]
res = 320x400
blitter = scanlines
driver = auto

[TV Mode]
res = 320x400
blitter = tvmode
driver = auto

;[TV Mode Doubled]
;res = 512x384
;blitter = tvmode_double
;driver = auto

[Eagle]
res = 640x480
blitter = eagle
driver = auto

;[Parallel]
;res = 640x480
;blitter = parallel
;driver = auto

[Perfect]
res = 512x384
blitter = tvmode_double
flip
vsync
driver = auto

